CPE 301: Lab 2

Terence Henriod

Section 1101

Instructor: Dr. Egbert

TA: Andy Olson

September 9, 2013

What minimum oscilloscope performance is required to properly capture 2 msec of a 1 Vpk-pk , 250 MHz sine wave?

1. Bandwidth:
2. Sample Rate:
3. Record Length: